# Wirtgen Surface Miners – Limestone mining without drilling and blasting in Ukraine

**Wirtgen surface miners play a key role in increasing production and reducing costs in material extraction for a large cement plant in Ukraine.**

PJSC Ivano-Frankivskcement (IFCEM) produces clinker and 300 other cement and gypsum products. The raw material for the cement plant comes from a deposit located 15 km to the north. The Carpathian mining area is rich in sedimentary rocks such as limestone, marl and gypsum.

**Production increase thanks to Wirtgen technologies**

For years, the material was extracted by drilling and blasting and then wet-processed into clinker in the cement plant. In a move to increase productivity and reduce costs, IFCEM became the first cement plant in the Ukraine to initiate the transition from the wet to the dry process, a measure which was accompanied by an optimization of the mining method for material supply.

The dry process is now considered the preferred method for clinker production as it reduces fuel consumption per ton of material. This in turn has a positive effect on production, costs and the environment. For an optimal drying process, the material from the quarry should only have a low moisture content so that it can be crushed in a dry crusher, ground to powder in the raw mill and burnt in the rotary kiln without further pre-treatment.

**Optimum exploitation of deposits, better raw material**

In order to ensure that the material extracted from the quarry is as dry as possible, a radical change in the mining method was necessary. Meanwhile, the previous use of explosives for limestone mining was having a detrimental effect on neighboring residential areas due to the noise generated and the ground vibrations. IFCEM found the solution in Wirtgen surface miner technology: In 2012, the company purchased a 2200 SM, in 2015 a second, identical model and in 2017 a 2500 SM.

By gradually phasing out the drilling and blasting operations, the surface miners progressively reduced the time and cost involved in pre-crushing and post-crushing the material and also made it possible to redesign the deposit. By ensuring a defined slope of the surface with the aid of the Level Pro automatic leveling system, the surface miners created the conditions for efficient dewatering.

Compared to drilling and blasting, this allows much drier raw material to be mined and the material can enter the plant's drying process without any further treatment. Thanks to the redesign of the mining area with the surface miner, the exploitation of the deposits has also been increased, because now even previously unused areas can be worked and additional material extracted.

**Economical and reliable surface miner trio**

The increased mining volume thus also had a major influence on the selection of the third machine model. After the impressive results of the smallest Wirtgen surface miner 2200 SM with a 2.2-m cutting drum and a cutting depth of up to 300 mm, the technical management of Ivano-Frankivskcement now opted for the even more powerful model, the 2500 SM.

Together, the three Wirtgen surface miners generate a daily output of 7,000 tons, which also leads to optimum utilization of the cement plant. The 2500 SM has made an important contribution to this, as well as to increasing production in the limestone quarries, where the material has a uniaxial compressive strength of between 20 and 70 MPa depending on its depth. The 2500 SM, which has already clocked more than 4,500 hours, is equipped with a 2.5 m-wide cutting drum fitted with cutting tools on an HT 15 quick-change tool-holder system. HT 15 reduces the time required to replace the tool-holder from 90 to 15 minutes compared to conventional welded tool-holder systems.

The 2500 SM, which can remove material up to 650 mm deep, extracts the material in Ivano-Frankivsk up to a depth of 40-45 cm. Depending on the rock hardness, the surface miner achieves a feed rate of 5 m per minute and a grain size of 0-100 mm. Depending on the hardness of the rock, the entire tooling is replaced at intervals that vary between 200 and 500 hours based on the machine's field of application.

**2500 SM: Performance and precision count**

Since its market launch, the 2500 SM has proven its performance and flexibility worldwide, as it can be used for the selective mining of raw materials with uniaxial compressive strength up to 80 MPa and in special cases even higher. The surface miner cuts, crushes and loads the rock in a single operation. Depending on the application, the material can either be loaded directly into trucks via the 11.3 m long, slewing discharge conveyor of the miner, deposited laterally or as a windrow between the machine's crawler tracks. The 2500 SM is powered by a 783-kW (1,065-HP) engine and features precise mining of the useful minerals thanks to the Level Pro leveling system integrated into the machine's control system.

The operator sits in a spacious, sound- and dustproof, air-conditioned cabin. A video system with several cameras gives the operator a complete overview during the extraction process, ensuring maximum safety. Machine operator Svyatoslav Podolyak, who together with Voladymyr Sauchut has been driving the 2500 SM since last year, sums up the advantages: "This surface miner has an excellent production rate, which is even higher than that of the 2200 SM. And that was already very good. Thanks to the clearly arranged instruments, I have all important information at a glance. The soundproofed and air-conditioned cabin also gives me an optimal view of the cutting edge and allows me to concentrate on my work in the cold winters and hot summers typical of this region.

**Surface miners get on track for an efficient production cycle**

According to Yaroslav Nesterovych Voznyak, Technical Manager of the deposit, the surface miners, especially the 2500 SM, have had a positive influence on the production cycle in the quarry and thus also in the cement plant: "The purchase of the Wirtgen surface miners made the transition from drilling and blasting to a safe mining process easy to implement. In addition to the environmental and production benefits, the surface miners have proven to be the best solution, especially in terms of cost efficiency and economical operation. The grain size of the material produced is ideal for the cement plant. This is why our fleet of surface miners will grow. We are already preparing a further mining area with a volume of around 180 million tons of material, which we want to mine with our Wirtgen surface miners".

Photos:

|  |  |
| --- | --- |
|  | W\_photo\_2500SM\_00894\_PR Avoiding blasting means avoiding danger. The use of Wirtgen surface miners significantly reduces noise and dust emissions as well as ground vibrations. |

|  |  |
| --- | --- |
|  | W\_photo\_2500SM\_00910\_PR For direct loading, Wirtgen surface miners and trucks generally travel in parallel in the same direction. However, the mine logistics in Yamnytsia required the truck to be positioned facing the opposite direction to the 2500 SM during loading. Thanks to the optimum visual concept of the surface miners, the operator was also able to load the material safely under these conditions. |

|  |  |
| --- | --- |
|  | W\_photo\_2500SM\_00897\_PR The surface miner 2500 SM from Wirtgen is used for the selective mining of raw materials with uniaxial compressive strengths of up to 80 MPa. It cuts, crushes and loads rock in a single operation. The economical and environmentally friendly process also creates stable, precise cutting surfaces which can be immediately traveled on by trucks.. |

Photos:

|  |  |
| --- | --- |
|  | W\_photo\_2500SM\_00933\_PR For Jaroslaw Nesterovych Voznyak, Technical Manager at IFCEM, the surface miners are the decisive factor for the optimized production cycle in the quarry: "The purchase of the Wirtgen surface miners has not only changed the mining method, but also had a significant positive impact on production in the cement plant. |

|  |  |
| --- | --- |
|  | W\_photo\_2500SM\_00931\_PR Machine operator Svyatoslav Podolyak points out the comfort of the 2500 SM. Equipped with large glass windows, the cab offers good visibility, ergonomic design and easy operation - giving the operator full control over the entire dismantling process. |

*Note: These photographs are only intended as a preview. For printing in publications, please use the photographs in 300 dpi resolution that are available for download from the Wirtgen GmbH / Wirtgen Group websites.*

|  |  |
| --- | --- |
| For further information  please contact:  WIRTGEN GmbH  Corporate Communications  Michaela Adams, Mario Linnemann  Reinhard-Wirtgen-Strasse 2  53578 Windhagen  Germany  Phone: +49 (0) 2645 131 – 4510  Fax: +49 (0) 2645 131 – 499  E-mail: presse@wirtgen.com  www.wirtgen.com |  |