Wirtgen Limited showcases innovative solutions for road construction and rehabilitation at Plantworx

**Presenting eight machines, the Wirtgen Group sales and service company Wirtgen Limited will be showcasing innovative solutions for road construction and rehabilitation at the Plantworx trade show. Alongside the key exhibit, the W 50 Ri, which is Wirtgen's latest 50-cm milling machine, visitors can also view two "Dash 3" generation pavers from Vögele and five rollers from the compaction specialist, Hamm.**

The W 50 Ri is a member of Wirtgen's new small milling machine generation and will be unveiled to trade experts at the show. The entirely new and striking design harbors a cornucopia of technical innovations that result in enhanced performance, greater productivity and maximum ease-of-operation. Wirtgen's brand new in-house development LEVEL PRO PLUS (a leveling system), which is fully integrated in the machine control system, supports intuitive and simple operation to produce precise and high-quality milling results. The generous locking angle on either side and the automatic tracking function of the rear inner wheel when folded in result in extremely small turning radii that make working on cramped job sites so much easier. Moreover three individually variable milling drum speeds each ensure an ideal milling performance for a broad range of applications. The fact that using the W 50 Ri can speed up completion of a project by as much as 20% makes this cold milling machine a key factor for success in road rehabilitation.

Vögele pavers and Hamm rollers also guarantee success on the job site – for instance the Vögele SUPER 800-3i from the Mini Class and the SUPER 1303-3i from the Compact Class, the Hamm compactor H 13i or the tandem rollers HD 8 VV, HD 12 VV, HD 13 VV and HD+ 90 VVi. Wirtgen Limited will also be presenting these machines to visitors in Leicestershire.

--------

**Fotos:**

|  |  |
| --- | --- |
| W50Ri_01223_HI | *W50Ri\_01223\_HI*  The systems for loading milled material on the Wirtgen W 50 Ri have been thoroughly optimized to maximize performance as well as functionality. A large slewing angle of 30° to the left and right, handy quick-change coupling and the hydraulically operated folding conveyor greatly facilitate the work process. |

--------

**For more information, please contact:**

Wirtgen Group   
Corporate Communications  
Michaela Adams, Mario Linnemann Reinhard-Wirtgen-Strasse 2   
53578 Windhagen   
Germany

Phone: +49 – 26 45 – 1 31 – 0   
Fax: +49 – 26 45 – 1 31 – 4 99   
E-Mail: presse@wirtgen.de

Internet: www.wirtgen-group.com