**Vögele │ Market launch for new mini road paver**

**SUPER 800-5 P-Tier with numerous innovations**

**Vögele has brought the first mini paver of the Dash 5 to market. With its new material hopper, new paver operator's platform and new lighting concept, the SUPER 800-5 P offers a high level of operating comfort and optimum visibility.**

**Focus on user-friendly operation**

As with all pavers of the Dash 5 generation, Vögele also focuses on high operating convenience and short set-up times with the new SUPER 800-5 P. In combination with the AB 200 V and TV and AB 220 V and TV extending screeds, it offers pave widths from 0.5 m to 3.5 m – making it ideal for narrow construction projects. The successor to the SUPER 700 and SUPER 800 has an engine output of 55.4 kW, a laydown rate of up to 300 tonnes per hour and is extremely compact with a width of 1.4 m and a length of 4.4 m. Compared to its predecessors, the Dash 5 model also integrates numerous practical innovations.

**New material hopper with double folding mechanism**

A major advantage of the mini paver is the newly developed material hopper: as before, both hopper walls can be hydraulically adjusted separately or together. In addition, the asymmetrical setting, for example for paving along a wall, can now be realised on both sides. The hopper walls of the new SUPER 800-5 P can also be folded twice. Together with the flat engine hood, the low hopper height and the raised operator's platform, this gives the operator an unrestricted view to the front. This makes manoeuvring and loading the new Dash 5 paver much easier.

**ErgoBasic 5 offers more flexibility and better ergonomics**

Vögele has also improved the operating system: as before, the new operator's control console can be moved horizontally. In addition, its angle can now be adjusted in four stages and ergonomically adapted to the height of the operator. The new ErgoBasic 5 operating concept follows the operating logic of the larger machines but has been specially adapted to the mini paver. For the first time, the paver operator's console incorporates a display that allows the operator to view the machine's operating data. In addition, Vögele has fully integrated the operation of the Auto Grade Basic system for automated grade and slope control into the screed control system. This enables screed operators to control the SUPER 800-5 P with just one compact console - just like on large Vögele pavers. A new storage system with a tool and drink holder, coat hooks, and 24-volt socket for mobile devices also ensures organization and more convenience.

**New lighting concept for optimum visibility**

With Light Package or Light Package Plus of the Dash 5 generation, users can pave safely, relaxed and precisely even in the dark or in poor visibility conditions. The light package for the SUPER 800-5 P includes LED lighting for the paver operator's console, the tow point cylinder and the auger tunnel. This ensures that all points relevant to the paving are specifically illuminated without casting shadows. The optional Light Package Plus also offers two LED floodlights that optimally illuminate the entire working area.

**Photos:**

  
**JV\_New\_SUPER\_800-5\_P\_001\_PR**

Better visibility, more order, more convenience: The new SUPER 800-5 P min paver from Vögele offers numerous advantages.

  
**JV\_New\_SUPER\_800-5\_P\_002\_PR**

Hinges in two ways: The material hopper of the SUPER 800-5 P gives the operator an unrestricted view to the front. This makes manoeuvring and loading the new Dash 5 paver much easier.

  
**JV\_New\_SUPER\_800-5\_P\_003\_PR**

New operating concept ErgoBasic 5: For the first time, the paver operator's console incorporates a display that allows the operator to view the machine's operating data.

*Note: The photographs shown here are only previews. If you wish to publish them in other media, please download the higher resolution (300 dpi) versions from the Wirtgen Group websites.*

**For further information, please contact us at:**

WIRTGEN GROUP

Public Relations

Reinhard-Wirtgen-Strasse 2

53578 Windhagen

Germany

Telephone: +49 (0) 2645 131 – 1966

Fax: +49 (0) 2645 131 – 499

Email: PR@wirtgen-group.com

[www.wirtgen-group.com](https://www.wirtgen-group.com)