**KLEEMANN** | **Higher application diversity for cone and impact crushers**

**Double-deck post screening unit for the MOBICONE MCO 90(i) EVO2 and MOBIREX MR 110(i) EVO2**

**The mobile cone crusher MOBICONE MCO 90(i) EVO2 and the mobile impact crusher MOBIREX MR 110(i) EVO2 can now be fitted with a double-deck post screening unit as an option.**

Cone crushers are mainly used in hard stone, impact crushers in soft to medium-hard stone and in recycling. A very high product quality is expected from both plant types. Thanks to the new optional double-deck post screening unit, it is now also possible, with a single machine – without the use of an additional screening plant – to produce two classified final grain sizes.

**Double-deck post screening unit guarantees high application diversity and flexibility**

The large screening surface makes effective screening possible even for grain sizes below 20 mm. The discharge height of the fine grain conveyor is designed for a maximum stockpile volume. Oversize grain can be processed in a closed material circuit via a return conveyor. As an option, the conveyor can be swivelled hydraulically by up to 100°, which also makes side discharge possible. A kidney-shaped stockpile can thus be created manually.

If an application is only to produce one classified final grain size, the post screening unit can simply be used as a single-deck version.

**Wind sifters for effective cleaning**

As the MOBIREX MR 110(i) EVO2 is frequently used in recycling applications, wind sifters are used here as an option. They guarantee increased material quality because contamination through lightweight material (e.g. wood and plastic) is removed from the material. The air flow can then be controlled precisely depending on the material. This also reduces manual and sorting work. The wind sifter can only be used in conjunction with the post screening unit. With the double-deck post screening unit, a second wind sifter can be used as an option for cleaning the medium grain.

Photo:



**KL\_Double-deck post screening unit**

The MOBICONE MCO 90(i) EVO2 and MOBIREX MR 110(i) EVO2 can now be equipped with an optional double-deck post screening unit.

*Note: This photo only serves as a preview. For printing in the publications, please use the photo in 300 dpi resolution which is available for downloading on the web pages of Wirtgen Group.*

|  |  |
| --- | --- |
| Further information  is available from:  WIRTGEN GROUP  Public Relations  Reinhard-Wirtgen-Straße 2  53578 Windhagen  Germany  Telephone: +49 (0) 2645 131 – 1966  Fax: +49 (0) 2645 131 – 499  E-mail: PR@wirtgen-group.com  www.wirtgen-group.com |  |